
---------- D:\ACADWIN\SUPPORT\HF.LSP
;d;;;;;;;;;;;;;;;;;;;;;;;;;;; Synthetic CAD ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;d; This is the programing documentation related to the creation of a Fuction
;d; Representaion modeling 3D party package of software for AutoCAD rel12
;d; with AME. The use of AutoLSP to model some of the problems associated 
;d; with the development of Synthetic CAD does not constitute using or 
;d; reproducing any of the features of the AutoCAD software interface.  
;d; The use of AutoCAD or AutoLSP software is for temporary research and in 
;d; the near term AutoCAD will be replaced. .
;d;
;d; First written by Hiroyuki Nifuku under GGPL modifyed by Carl Vilbrandt
;d;
;d; ------------------------ Hyper Fun Get ------------------------ 
;d; 
;d; Hyper_Fun_Get (HFG) You select one csg-obj at a time for conversion.
;d; * change to multa selection processes.
;d; HFG processes CSG data: is a box, cone, cylinder, sphere or Torus
;d; The follow HFG vars and notes on programs:
;d; 
;d; obj: 1536 = box, 1537 = cone,1538 =cylinder, 1539 =sphere, 1540 = torus
;d;  
;d; objdata: contains all of the selected objects:
;d;          1. It might slow down the system if it gets large but I don't
;d;             think so.
;d;          2. It is only in RAM & VRAM so the work is lost on shutdown.
;d;          3. It only works with CSG prim...So we will need to create Xtended
;d;             data structure for HF anyway. 
;d;   
;d;;;;;;;;; Make HyperFun (HFM) program ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;d; You enter file name and it creates a hyperfun file.
;d;;;;;;;;;;;;;;;;;;;;;;;;; HF_Del hf_data.dat ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
